Fast Amp PCB Manufacturing Instructions

University of Pennsylvania, Dept. of Physics and Astronomy

BOARD NAME: FAST AMP

DATE: August 28, 2017

CONTACTS:

Emmanuel Morales: silver\_morales2@hotmail.com

Mitch Newcomer: mitch@hep.upenn.edu

Mike Reilly: mbreilly@hep.upenn.edu

MANUFACTURING NOTES

1. This is a 4 layer board with the following order:

TOP

GND

POWER

BOTTOM

1. MATERIAL: FR4
2. BOARD THICKNESS: 62 mils
3. COPPER THICKNESS: all layers 1oz copper.
4. All holes plated through unless otherwise noted.
5. FINISH: immersion gold