Field & Power vs. I.R. of Cu Magnet with 30-cm Build or 50-cm O.R.

Robert J. Weggel; Magnet Optimization Research Engineering (M.O.R.E.), LLC; 1/13/2014



Fig. 1. Outer radius, power, current & field contribution (in 15-T background field) vs. inner radius of magnet with 10 layers (30-cm radial depth) of JHF-like mineral-insulated conductor. In every layer the peak hot-spot temperature is 90 ºC at 10 ºC inlet temperature, 40-atm water pressure, and three hydraulic passages per layer.



Fig. 2. Power & field contribution (in 15-T background field) vs. inner radius of 50-cm-O.R. magnet of JHF-like mineral-insulated conductor. In every layer the peak hot-spot temperature is 90 ºC with an inlet temperature of 10 ºC inlet temperature, a water-pressure drop of 40 atmospheres, and three hydraulic passages per layer.



Fig. 3. Power & field contribution (in 15-T background field) vs. inner radius of the most-efficient 50-cm-O.R. magnet of JHF-like mineral-insulated conductor. In each layer the peak hot-spot temperature is 90 ºC or less with an inlet temperature of 10 ºC, a water-pressure drop of 40 atmospheres, and three hydraulic passages per layer. Emphasizing efficiency instead of maximum possible field saves considerable power with only modest sacrifice in field.



Fig. 4. Power & field contribution (in 15-T background field) vs. inner radius of the most-efficient 10-MW magnet with 30-cm radial depth of windings of JHF-like mineral-insulated conductor. In each layer the peak hot-spot temperature is 90 ºC or less with an inlet temperature of 10 ºC, a water-pressure drop of 40 atmospheres, and three hydraulic passages per layer.